/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16Ball"
/ File opened for write Tue May 07 12:21:34 2013.
identifier name "F16Ball" new saveprevious
import acis "D:\\AirplaneModel\\F16Jitou\\Jitou.sat" ascii
volume create width 20 depth 8 height 8 brick
volume move "volume.2" offset -50 0 0
undo
/Undone to: volume move "volume.2" offset -50 0 0
volume move "volume.2" offset 5 0 0
undo
/Undone to: volume move "volume.2" offset 5 0 0
volume move "volume.2" offset -5 0 0
volume move "volume.2" offset 0 3 0
undo
/Undone to: volume move "volume.2" offset 0 3 0
volume move "volume.2" offset 0 2 0
undo
/Undone to: volume move "volume.2" offset 0 2 0
volume move "volume.2" offset 0 1 0
/ERROR occurred in the next command!
face mesh "face.1" "face.2" "face.3" "face.4" "face.5" "face.6" "face.7" \
  triprimitive size 0.02
face mesh "face.1" "face.2" "face.3" "face.4" "face.5" "face.6" "face.7" pave \
  size 0.02
volume create radius 0.05 sphere
volume move "volume.3" offset -5 0 0
volume move "volume.3" offset 0.5 0.8 0
undo
/Undone to: volume move "volume.3" offset 0.5 0.8 0
volume move "volume.3" offset 0.5 0.4 0
volume cmove "volume.3" multiple 1 offset 0 4 0
volume cmove "volume.4" multiple 1 offset 0 -2 0
volume delete "volume.4" lowertopology
volume cmove "volume.5" multiple 1 offset 0 0 3
volume cmove "volume.5" multiple 1 offset 0 0 -3
volume cmove "volume.3" multiple 1 offset -8 0 0
face mesh "face.19" "face.14" "face.16" "face.17" "face.18" pave size 0.01
face mesh "face.10" map size 0.4
undo
/Undone to: face mesh "face.10" map size 0.4
face mesh "face.13" "face.8" "face.12" "face.9" map size 0.3
volume mesh "volume.2" tetrahedral size 0.1
undo
/Undone to: volume mesh "volume.2" tetrahedral size 0.1
undo
/Undone to: face mesh "face.13" "face.8" "face.12" "face.9" map size 0.3
face mesh "face.10" map size 0.2
undo begingroup
edge picklink "edge.22" "edge.14" "edge.17" "edge.25"
edge mesh "edge.25" "edge.17" "edge.14" "edge.22" successive ratio1 1 \
  intervals 50
undo endgroup
physics create "inlet" btype "VELOCITY_INLET" face "face.10"
physics create "outlet" btype "PRESSURE_OUTLET" face "face.12" "face.13" \
  "face.8" "face.9" "face.11"
physics create "AIR" ctype "FLUID" volume "volume.2"
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16Ball"
/ File opened for append Tue May 07 13:53:01 2013.
physics delete "outlet" btype
physics create "outlet" btype "PRESSURE_OUTLET" face "face.11"
physics create "profile" btype "VELOCITY_INLET" face "face.12" "face.13" \
  "face.8" "face.9"
save
face mesh "face.11" map size 0.2
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16Ball"
/ File opened for append Tue May 07 15:09:17 2013.
volume delete "volume.8" lowertopology
volume delete "volume.3" "volume.5" "volume.6" "volume.7" lowertopology
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16Ball"
/ File opened for append Wed May 08 15:41:40 2013.
save name "F16z.dbs"
face delete "face.11" lowertopology onlymesh
undo begingroup
edge delete "edge.25" "edge.22" "edge.14" "edge.17" keepsettings onlymesh
edge mesh "edge.25" "edge.22" "edge.14" "edge.17" successive ratio1 \
  0.98039216 ratio2 0.98039216 intervals 120
undo endgroup
save
volume create height 0.4 radius1 0.72 radius3 0.2 offset -0.2 0 0 xaxis frustum
undo
/Undone to: volume create height 0.4 radius1 0.72 radius3 0.2 offset -0.2 0 0 xax
volume create height 0.4 radius1 0.36 radius3 0.1 offset -0.2 0 0 xaxis frustum
undo
/Undone to: volume create height 0.4 radius1 0.36 radius3 0.1 offset -0.2 0 0 xax
volume create height 0.2 radius1 0.36 radius3 0.1 offset 0.1 0 0 xaxis frustum
vertex create coordinates 0.2 0 0
vertex create coordinates 0.3 0.05 0
undo
/Undone to: vertex create coordinates 0.3 0.05 0
vertex create coordinates 0.3 0.01 0
vertex create coordinates 0.4 0.02 0
undo
/Undone to: vertex create coordinates 0.4 0.02 0
undo
/Undone to: vertex create coordinates 0.3 0.01 0
vertex create coordinates 0.3 0.04 0
undo
/Undone to: vertex create coordinates 0.3 0.04 0
vertex create coordinates 0.3 0.02 0
vertex create coordinates 0.4 0.05 0
vertex create coordinates 0.5 0.08 0
vertex create coordinates 0.7 0.12 0
undo
/Undone to: vertex create coordinates 0.7 0.12 0
vertex create coordinates 0.6 0.12 0
vertex create coordinates 0.7 0.18 0
vertex create coordinates 0.8 0.25 0
edge create nurbs "vertex.21" "vertex.22" "vertex.23" "vertex.24" "vertex.25" \
  "vertex.26" "vertex.27" interpolate
volume create translate "face.16" onedge "edge.28"
window modify shade
window modify shade
default set "GRAPHICS.GENERAL.CONNECTIVITY_BASED_COLORING" numeric 1
window modify shade
window modify shade
window modify noshade
default set "GRAPHICS.GENERAL.CONNECTIVITY_BASED_COLORING" numeric 0
undo
/Undone to: default set "GRAPHICS.GENERAL.CONNECTIVITY_BASED_COLORING" numeric 0
undo
/Undone to: default set "GRAPHICS.GENERAL.CONNECTIVITY_BASED_COLORING" numeric 1
undo
/Undone to: volume create translate "face.16" onedge "edge.28"
undo
/Undone to: edge create nurbs "vertex.21" "vertex.22" "vertex.23" "vertex.24" "ve
redo
volume create height 0.05 radius1 0.25 radius3 0.1 offset 0.025 0 0 xaxis frustum
volume delete "volume.3" lowertopology
undo
/Undone to: volume delete "volume.3" lowertopology
undo
/Undone to: volume create height 0.05 radius1 0.25 radius3 0.1 offset 0.025 0 0 x
volume create height 0.8 radius1 0.25 radius3 0.1 offset 0.4 0 0 xaxis frustum
undo
/Undone to: volume create height 0.8 radius1 0.25 radius3 0.1 offset 0.4 0 0 xaxi
volume create height 0.05 radius1 0.25 radius3 0.1 offset 0.025 0 0 xaxis frustum
volume delete "volume.3" lowertopology
volume create height 0.15 radius1 0.1 radius3 0.05 offset 0.075 0 0 xaxis frustum
undo
/Undone to: volume create height 0.15 radius1 0.1 radius3 0.05 offset 0.075 0 0 x
volume create height 0.15 radius1 0.1 radius3 0.03 offset 0.075 0 0 xaxis frustum
volume move "volume.5" offset 0.05 0 0
edge delete "edge.28" lowertopology
undo
/Undone to: edge delete "edge.28" lowertopology
undo
/Undone to: volume move "volume.5" offset 0.05 0 0
undo
/Undone to: volume create height 0.15 radius1 0.1 radius3 0.03 offset 0.075 0 0 x
volume create height 0.15 radius1 0.1 radius3 0.06 offset 0.075 0 0 xaxis frustum
volume move "volume.5" offset 0.05 0 0
undo
/Undone to: volume move "volume.5" offset 0.05 0 0
undo
/Undone to: volume create height 0.15 radius1 0.1 radius3 0.06 offset 0.075 0 0 x
volume create height 0.15 radius1 0.1 radius3 0.05 offset 0.075 0 0 xaxis frustum
volume move "volume.5" offset 0.05 0 0
volume create height 0.1 radius1 0.03 radius3 0.03 offset 0 0 0.05 zaxis frustum
undo
/Undone to: volume create height 0.1 radius1 0.03 radius3 0.03 offset 0 0 0.05 za
volume create height 0.1 radius1 0.03 radius3 0.03 offset 0.05 0 0 xaxis frustum
volume move "volume.6" offset 0.2 0 0
edge delete "edge.28" lowertopology
volume move "volume.6" offset 0.2 0 0
volume create height 0.25 radius1 0.05 radius3 0.03 offset 0.125 0 0 xaxis frustum
volume move "volume.7" offset 0.2 0 0
volume delete "volume.6" lowertopology
volume create radius 0.03 sphere
volume move "volume.8" offset 0.45 0 0
vertex delete "vertex.22" "vertex.23" "vertex.24" "vertex.25" "vertex.26" \
  "vertex.31" "vertex.34" "vertex.35"
vertex delete "vertex.6" "vertex.7"
volume unite volumes "volume.8" "volume.7" "volume.5" "volume.4"
volume reflect "volume.8" vector 1 0 0 origin 0 0 0
volume move "volume.8" offset -5 0.8 0
volume move "volume.8" offset 0 0.06 0
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z"
/ File opened for append Wed May 08 16:52:56 2013.
physics create "ZT" btype "WALL" face "face.17" "face.19" "face.21" "face.27" \
  "face.29"
physics create "Body" btype "WALL" face "face.1" "face.2" "face.3" "face.4" \
  "face.5" "face.6" "face.7"
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z"
/ File opened for append Wed May 08 17:09:51 2013.
identifier name "D:\\AirplaneModel\\F16ZhuiTao\\F16z.dbs" old saveprevious
volume move "volume.8" offset 0.25 0 0
save
volume move "volume.8" offset -0.25 0 0
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z"
/ File opened for append Thu May 09 19:50:10 2013.
volume delete "volume.2" lowertopology
volume split "volume.8" faces "face.21" connected
undo
/Undone to: volume split "volume.8" faces "face.21" connected
undo
/Undone to: volume delete "volume.2" lowertopology
undo
redo
face create wireframe "edge.31" real
volume split "volume.8" faces "face.30" connected
volume delete "volume.8" lowertopology
volume move "volume.9" offset 5 0 0
volume move "volume.9" offset 0 -0.86 0
volume create radius1 0.35 radius2 0.05 zaxis torus
undo
/Undone to: volume create radius1 0.35 radius2 0.05 zaxis torus
volume create radius1 0.35 radius2 0.02 xaxis torus
volume move "volume.9" offset -0.2 0 0
volume move "volume.10" "volume.9" offset -5 0 0
volume move "volume.10" "volume.9" offset 0 0.86 0
vertex create onface "face.31" uparameter -0.8182033 vparameter 1.2040446
vertex delete "vertex.37"
vertex create onface "face.31" uparameter -2.7011843 vparameter 6.1230318e-17
vertex cmove "vertex.30" multiple 1 offset 0 -0.01 0
edge create straight "vertex.38" "vertex.37"
face create radius 0.01 yzplane circle
vertex create coordinates 0 0 0
face align "face.32" translation "vertex.40" "vertex.38"
edge create translate "vertex.37" onedge "edge.38"
edge merge "edge.38" "edge.40" forced
volume create translate "face.32" onedge "edge.38"
window modify shade
window modify noshade
volume intersect volumes "volume.11" "volume.10" keeporiginals
volume subtract "volume.11" volumes "volume.12"
undo
/Undone to: volume subtract "volume.11" volumes "volume.12"
volume subtract "volume.11" volumes "volume.12"
undo
/Undone to: volume subtract "volume.11" volumes "volume.12"
volume subtract "volume.11" volumes "volume.12" keeptool
volume delete "volume.11" lowertopology
edge delete "edge.38" lowertopology
volume delete "volume.12" lowertopology
volume move "volume.10" "volume.13" "volume.9" offset 0 -0.86 0
volume cmove "volume.13" multiple 1 dangle 45 vector 1 0 0 origin 0 0 0
volume cmove "volume.14" multiple 1 dangle 45 vector 1 0 0 origin 0 0 0
volume cmove "volume.15" multiple 1 dangle 45 vector 1 0 0 origin 0 0 0
volume cmove "volume.16" multiple 1 dangle 45 vector 1 0 0 origin 0 0 0
volume cmove "volume.17" multiple 1 dangle 45 vector 1 0 0 origin 0 0 0
volume cmove "volume.18" multiple 1 dangle 45 vector 1 0 0 origin 0 0 0
volume cmove "volume.19" multiple 1 dangle 45 vector 1 0 0 origin 0 0 0
window modify noshade
default set "GRAPHICS.GENERAL.CONNECTIVITY_BASED_COLORING" numeric 1
default set "GRAPHICS.GENERAL.CONNECTIVITY_BASED_COLORING" numeric 0
window modify shade
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z"
/ File opened for append Thu May 09 20:17:25 2013.
identifier name "D:\\AirplaneModel\\F16ZTGaiJin\\F16z.dbs" old saveprevious
volume create radius1 0.35 radius2 0.04 xaxis torus
undo
/Undone to: volume create radius1 0.35 radius2 0.04 xaxis torus
volume create radius1 0.32 radius2 0.04 xaxis torus
volume cmove "volume.1" multiple 1 offset 0 2 0
volume delete "volume.1" lowertopology
vertex delete "vertex.5"
volume create width 0.4 depth 1 height 1 brick
volume cmove "volume.23" multiple 1 offset -0.2 0 0
volume delete "volume.23" lowertopology
volume subtract "volume.21" volumes "volume.24" keeptool
volume delete "volume.24" lowertopology
volume cmove "volume.21" multiple 1 offset -5 0 0
volume delete "volume.21" lowertopology
volume delete "volume.10" lowertopology
volume delete "volume.15" "volume.16" "volume.14" "volume.13" "volume.18" \
  "volume.20" lowertopology
volume delete "volume.17" lowertopology
undo
/Undone to: volume delete "volume.17" lowertopology
undo
/Undone to: volume delete "volume.15" "volume.16" "volume.14" "volume.13" "volume
undo
/Undone to: volume delete "volume.10" lowertopology
undo
/Undone to: volume delete "volume.21" lowertopology
undo
/Undone to: volume cmove "volume.21" multiple 1 offset -5 0 0
redo
redo
volume delete "volume.10" lowertopology
volume delete "volume.13" "volume.14" "volume.15" "volume.16" "volume.17" \
  "volume.18" "volume.19" "volume.20" lowertopology
vertex cmove "vertex.30" multiple 1 offset 0 -0.01 0
vertex create onedge "edge.114" percentarclength 0.75
vertex move "vertex.102" offset 0 -0.02 0
edge create straight "vertex.101" "vertex.102"
face create radius 0.01 yzplane circle
face align "face.96" translation "vertex.40" "vertex.101"
volume create translate "face.96" onedge "edge.115"
window modify shade
edge delete "edge.115" lowertopology
undo
/Undone to: edge delete "edge.115" lowertopology
undo
/Undone to: volume create translate "face.96" onedge "edge.115"
undo
/Undone to: face align "face.96" translation "vertex.40" "vertex.101"
undo
/Undone to: face create radius 0.01 yzplane circle
undo
/Undone to: edge create straight "vertex.101" "vertex.102"
undo
/Undone to: vertex move "vertex.102" offset 0 -0.02 0
vertex move "vertex.102" offset 0 -0.03 0
undo
/Undone to: vertex move "vertex.102" offset 0 -0.03 0
vertex move "vertex.102" offset 0 -0.04 0
edge create straight "vertex.101" "vertex.102"
face create radius 0.01 yzplane circle
face align "face.96" translation "vertex.40" "vertex.101"
volume create translate "face.96" onedge "edge.115"
edge delete "edge.115" lowertopology
window modify shade
volume cmove "volume.24" multiple 1 dangle 15 vector 1 0 0 origin 0 0 0
volume cmove "volume.25" multiple 1 dangle 15 vector 1 0 0 origin 0 0 0
volume cmove "volume.26" multiple 1 dangle 15 vector 1 0 0 origin 0 0 0
volume cmove "volume.27" "volume.26" "volume.25" "volume.24" multiple 1 \
  dangle 45 vector 1 0 0 origin 0 0 0
undo
/Undone to: volume cmove "volume.27" "volume.26" "volume.25" "volume.24" multiple
volume cmove "volume.27" "volume.26" "volume.25" "volume.24" multiple 1 \
  dangle 60 vector 1 0 0 origin 0 0 0
volume cmove "volume.28" "volume.29" "volume.30" "volume.31" multiple 1 \
  dangle 60 vector 1 0 0 origin 0 0 0
volume cmove "volume.32" "volume.33" "volume.34" "volume.35" multiple 1 \
  dangle 60 vector 1 0 0 origin 0 0 0
volume cmove "volume.36" "volume.37" "volume.38" "volume.39" multiple 1 \
  dangle 60 vector 1 0 0 origin 0 0 0
volume cmove "volume.40" "volume.41" "volume.42" "volume.43" multiple 1 \
  dangle 60 vector 1 0 0 origin 0 0 0
window modify shade
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z"
/ File opened for append Thu May 09 22:12:33 2013.
identifier name "D:\\AirplaneModel\\F16ZTGaiJin\\F16z.dbs" old nosaveprevious
volume delete "volume.25" "volume.27" "volume.30" "volume.28" "volume.34" \
  "volume.32" "volume.31" "volume.26" "volume.29" "volume.35" "volume.33" \
  "volume.39" "volume.38" "volume.36" "volume.37" "volume.43" "volume.42" \
  "volume.41" "volume.40" "volume.47" "volume.46" "volume.45" "volume.44" \
  lowertopology
volume cmove "volume.24" multiple 1 dangle 20 vector 1 0 0 origin 0 0 0
volume cmove "volume.25" multiple 1 dangle 20 vector 1 0 0 origin 0 0 0
volume cmove "volume.26" "volume.25" "volume.24" multiple 1 dangle 60 vector \
  1 0 0 origin 0 0 0
volume cmove "volume.27" "volume.28" "volume.29" multiple 1 dangle 60 vector \
  1 0 0 origin 0 0 0
volume cmove "volume.30" "volume.31" "volume.32" multiple 1 dangle 60 vector \
  1 0 0 origin 0 0 0
volume cmove "volume.35" "volume.34" "volume.33" multiple 1 dangle 60 vector \
  1 0 0 origin 0 0 0
volume cmove "volume.36" "volume.37" "volume.38" multiple 1 dangle 60 vector \
  1 0 0 origin 0 0 0
window modify shade
volume move "volume.22" offset 0 -2 0
save name "F16z2.dbs"
volume unite volumes "volume.9" "volume.23" "volume.24" "volume.25" \
  "volume.26" "volume.27" "volume.28" "volume.29" "volume.30" "volume.31" \
  "volume.32" "volume.33" "volume.34" "volume.35" "volume.36" "volume.37" \
  "volume.38" "volume.39" "volume.40" "volume.41"
volume move "volume.9" offset 0 0.9 0
volume move "volume.9" "volume.22" offset 0 -1 0
volume create width 12 depth 8 height 8 brick
volume move "volume.23" offset -3 0 0
physics delete btype
physics create "inlet" btype "VELOCITY_INLET" face "face.170"
physics create "outlet" btype "PRESSURE_OUTLET" face "face.171"
physics create "profile" btype "VELOCITY_INLET" face "face.172" "face.173" \
  "face.168" "face.169"
physics create "BZT" btype "WALL" face "face.21" "face.27" "face.29" \
  "face.94" "face.95" "face.97" "face.99" "face.102" "face.105" "face.108" \
  "face.111" "face.114" "face.117" "face.120" "face.123" "face.126" \
  "face.129" "face.132" "face.135" "face.138" "face.141" "face.144" \
  "face.147" "face.167"
physics create "Body" btype "WALL" face "face.67" "face.68" "face.69" \
  "face.70" "face.71" "face.72" "face.73"
physics modify "AIR" ctype volume "volume.23"
undo begingroup
edge picklink "edge.213" "edge.205" "edge.208" "edge.216"
edge mesh "edge.216" "edge.208" "edge.205" "edge.213" successive ratio1 \
  0.98039216 ratio2 0.98039216 intervals 60
undo endgroup
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z2"
/ File opened for append Thu May 09 22:24:41 2013.
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z2"
/ File opened for append Thu May 09 22:28:04 2013.
identifier name "D:\\AirplaneModel\\F16ZTGaiJin\\F16z2.dbs" old \
  nosaveprevious
save name "F16z3.dbs"
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z3"
/ File opened for append Thu May 09 22:49:50 2013.
volume delete "volume.9" lowertopology
import acis "D:\\AirplaneModel\\F16ZTGaiJin\\Zhuitao.sat" ascii
volume delete "volume.34" "volume.36" "volume.35" "volume.26" "volume.33" \
  "volume.31" "volume.28" "volume.25" "volume.29" "volume.27" "volume.32" \
  "volume.24" lowertopology
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z3"
/ File opened for append Thu May 09 22:54:02 2013.
identifier name "D:\\AirplaneModel\\F16ZTGaiJin\\F16z3.dbs" old saveprevious
physics modify "BZT" btype face "face.192" "face.193" "face.194" "face.195" \
  "face.211" "face.212"
save
/ File closed at Thu May 09 22:54:32 2013, 0.56 cpu second(s), 552604376 maximum memory.
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z3"
/ File opened for append Fri May 10 10:11:01 2013.
volume create radius1 0.33 radius2 0.04 zaxis torus
undo
/Undone to: volume create radius1 0.33 radius2 0.04 zaxis torus
volume create radius1 0.33 radius2 0.04 xaxis torus
undo
/Undone to: volume create radius1 0.33 radius2 0.04 xaxis torus
volume create radius1 0.32 radius2 0.05 xaxis torus
volume create radius1 0.32 radius2 0.03 xaxis torus
volume move "volume.39" offset 0.01 0 0
volume subtract "volume.38" volumes "volume.39"
volume create width 1 depth 1 height 1 brick
volume move "volume.39" offset -0.5 0 0
volume subtract "volume.38" volumes "volume.39"
volume delete "volume.23" lowertopology
window modify shade
undo
/Undone to: volume delete "volume.23" lowertopology
volume delete "volume.37" lowertopology
volume move "volume.38" offset -5 0 0
save name "F16z7.dbs"
volume subtract "volume.23" volumes "volume.30" "volume.38"
/ERROR occurred in the next command!
face mesh "face.192" "face.193" "face.194" "face.195" "face.214" "face.221" \
  "face.222" "face.223" map size 0.01
face mesh "face.192" "face.193" "face.194" "face.195" "face.214" "face.221" \
  "face.222" "face.223" pave size 0.01
undo
/Undone to: face mesh "face.192" "face.193" "face.194" "face.195" "face.214" "fac
face mesh "face.214" "face.222" pave size 0.005
face mesh "face.192" "face.193" "face.194" "face.195" "face.214" "face.221" \
  "face.222" "face.223" pave size 0.01
volume mesh "volume.23" tetrahedral size 1
undo
/Undone to: volume mesh "volume.23" tetrahedral size 1
undo
/Undone to: face mesh "face.192" "face.193" "face.194" "face.195" "face.214" "fac
undo
/Undone to: face mesh "face.214" "face.222" pave size 0.005
undo
/Undone to: face mesh "face.192" "face.193" "face.194" "face.195" "face.214" "fac
undo
/Undone to: volume subtract "volume.23" volumes "volume.30" "volume.38"
undo
undo
undo
undo
undo
undo
physics modify "BZT" btype face "face.192" "face.193" "face.194" "face.195" \
  "face.223" "face.222" "face.221" "face.214"
physics modify "Body" btype face "face.67" "face.68" "face.69" "face.70" \
  "face.71" "face.72" "face.73"
save
/ File closed at Fri May 10 10:20:17 2013, 68.95 cpu second(s), 198661872 maximum memory.
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z7"
/ File opened for append Fri May 10 15:25:55 2013.
save name "F16z8.dbs"
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z8"
/ File opened for append Fri May 10 15:40:43 2013.
volume delete "volume.23" lowertopology
volume delete "volume.30" "volume.38" lowertopology
import acis "D:\\AirplaneModel\\F16ZT0510_1\\ZTMX.sat" ascii
volume move "volume.22" offset 0 0.14 0
volume create width 10 depth 6 height 6 brick
volume move "volume.24" offset -3 0 0
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z8"
/ File opened for append Fri May 10 16:55:29 2013.
physics delete btype
physics create "INLET" btype "VELOCITY_INLET" face "face.130" "face.132" \
  "face.128" "face.133" "face.129"
physics create "OUTLET" btype "VELOCITY_INLET" face "face.131"
physics create "BZT" btype "WALL" face "face.74" "face.75" "face.76" \
  "face.77" "face.78" "face.79" "face.80" "face.81" "face.82" "face.83" \
  "face.84" "face.85" "face.86" "face.87" "face.88" "face.89" "face.90" \
  "face.91" "face.92" "face.93" "face.94" "face.95" "face.96" "face.97" \
  "face.98" "face.99" "face.100" "face.101" "face.102" "face.103" "face.104" \
  "face.105" "face.106" "face.107" "face.108" "face.109" "face.110" \
  "face.111" "face.112" "face.113" "face.114" "face.115" "face.116" \
  "face.117" "face.118" "face.119" "face.120" "face.121" "face.122" \
  "face.123" "face.124" "face.125" "face.126" "face.127"
physics create "BODY" btype "WALL" face "face.67" "face.68" "face.69" \
  "face.70" "face.71" "face.72" "face.73"
physics modify "AIR" ctype volume "volume.24"
undo begingroup
edge picklink "edge.213" "edge.219" "edge.193" "edge.203" "edge.154" \
  "edge.155" "edge.108" "edge.98" "edge.88" "edge.81" "edge.79" "edge.76" \
  "edge.87" "edge.80" "edge.107" "edge.97" "edge.145" "edge.146" "edge.202" \
  "edge.192" "edge.218" "edge.212" "edge.223" "edge.220" "edge.187" \
  "edge.174" "edge.182" "edge.173" "edge.171" "edge.165" "edge.153" \
  "edge.152" "edge.130" "edge.136" "edge.119" "edge.128" "edge.113" \
  "edge.126" "edge.118" "edge.127" "edge.129" "edge.135" "edge.148" \
  "edge.149" "edge.170" "edge.164" "edge.181" "edge.172"
edge mesh "edge.172" "edge.181" "edge.164" "edge.170" "edge.149" "edge.148" \
  "edge.135" "edge.129" "edge.127" "edge.118" "edge.126" "edge.113" \
  "edge.128" "edge.119" "edge.136" "edge.130" "edge.152" "edge.153" \
  "edge.165" "edge.171" "edge.173" "edge.182" "edge.174" "edge.187" \
  "edge.220" "edge.223" "edge.212" "edge.218" "edge.192" "edge.202" \
  "edge.146" "edge.145" "edge.97" "edge.107" "edge.80" "edge.87" "edge.76" \
  "edge.79" "edge.81" "edge.88" "edge.98" "edge.108" "edge.155" "edge.154" \
  "edge.203" "edge.193" "edge.219" "edge.213" successive ratio1 1 intervals 2
undo endgroup
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z8"
/ File opened for append Fri May 10 17:58:04 2013.
identifier name "D:\\AirplaneModel\\F16ZT0510_1\\F16z8.dbs" old saveprevious
physics modify "OUTLET" btype "PRESSURE_OUTLET" face "face.131"
save
/ File closed at Fri May 10 17:58:31 2013, 0.52 cpu second(s), 482240840 maximum memory.
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z8"
/ File opened for append Fri May 10 19:11:45 2013.
volume subtract "volume.24" volumes "volume.22"
face mesh "face.67" "face.68" "face.69" "face.70" "face.71" "face.72" \
  "face.73" pave size 0.02
face mesh "face.128" "face.129" "face.130" "face.132" "face.133" "face.131" \
  map size 0.15
window modify invisible mesh
save
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z8"
/ File opened for append Sun May 12 12:29:07 2013.
/ File closed at Sun May 12 12:30:14 2013, 1.11 cpu second(s), 11938768 maximum memory.
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z8"
/ File opened for append Sun May 12 12:43:56 2013.
volume move "volume.23" offset 1.75 0 0
save name "F16z8s03_25.dbs"
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z8s03_25"
/ File opened for append Thu Oct 31 14:02:01 2013.
physics delete btype
physics create "inlet" btype "VELOCITY_INLET" face "face.130"
physics create "front" btype "VELOCITY_INLET" face "face.133"
physics create "down" btype "VELOCITY_INLET" face "face.129"
physics create "back" btype "PRESSURE_OUTLET" face "face.128"
physics create "outlet" btype "PRESSURE_OUTLET" face "face.131"
physics create "up" btype "PRESSURE_OUTLET" face "face.132"
physics create "ZT" btype "PRESSURE_OUTLET" face "face.74" "face.75" \
  "face.76" "face.77" "face.78" "face.79" "face.80" "face.81" "face.82" \
  "face.83" "face.84" "face.85" "face.86" "face.87" "face.88" "face.89" \
  "face.90" "face.91" "face.92" "face.93" "face.94" "face.95" "face.96" \
  "face.97" "face.98" "face.99" "face.100" "face.101" "face.102" "face.103" \
  "face.104" "face.105" "face.106" "face.107" "face.108" "face.109" \
  "face.110" "face.111" "face.112" "face.113" "face.114" "face.115" \
  "face.116" "face.117" "face.118" "face.119" "face.120" "face.121" \
  "face.122" "face.123" "face.124" "face.125" "face.126" "face.127"
physics modify "ZT" btype "WALL" face "face.74" "face.75" "face.76" "face.77" \
  "face.78" "face.79" "face.80" "face.81" "face.82" "face.83" "face.84" \
  "face.85" "face.86" "face.87" "face.88" "face.89" "face.90" "face.91" \
  "face.92" "face.93" "face.94" "face.95" "face.96" "face.97" "face.98" \
  "face.99" "face.100" "face.101" "face.102" "face.103" "face.104" "face.105" \
  "face.106" "face.107" "face.108" "face.109" "face.110" "face.111" \
  "face.112" "face.113" "face.114" "face.115" "face.116" "face.117" \
  "face.118" "face.119" "face.120" "face.121" "face.122" "face.123" \
  "face.124" "face.125" "face.126" "face.127"
physics create "BODY" btype "WALL" face "face.67" "face.68" "face.69" \
  "face.70" "face.71" "face.72" "face.73"
save
/ File closed at Thu Oct 31 14:06:13 2013, 9.81 cpu second(s), 11979440 maximum memory.
/ Journal File for GAMBIT 2.4.6, Database 2.4.4, ntx86 SP2007051421
/ Identifier "F16z8s03_25"
/ File opened for append Thu Oct 31 16:41:58 2013.
physics delete btype
physics create "inlet" btype "VELOCITY_INLET" face "face.130" "face.128" \
  "face.133"
physics create "outlet" btype "PRESSURE_OUTLET" face "face.131" "face.132" \
  "face.129"
physics create "Body" btype "WALL" face "face.67" "face.68" "face.69" \
  "face.70" "face.71" "face.72" "face.73"
physics create "ZT" btype "WALL" face "face.74" "face.75" "face.76" "face.77" \
  "face.78" "face.79" "face.80" "face.81" "face.82" "face.83" "face.84" \
  "face.85" "face.86" "face.87" "face.88" "face.89" "face.90" "face.91" \
  "face.92" "face.93" "face.94" "face.95" "face.96" "face.97" "face.98" \
  "face.99" "face.100" "face.101" "face.102" "face.103" "face.104" "face.105" \
  "face.106" "face.107" "face.108" "face.109" "face.110" "face.111" \
  "face.112" "face.113" "face.114" "face.115" "face.116" "face.117" \
  "face.118" "face.119" "face.120" "face.121" "face.122" "face.123" \
  "face.124" "face.125" "face.126" "face.127"
save
/ File closed at Thu Oct 31 16:50:26 2013, 7.97 cpu second(s), 11983032 maximum memory.
